

# [Testout 11](https://assignbuster.com/testout-11/)

If the SONET (oc-1) base data rate is 51. 84 mbps622. 08

To access the internet through the pstnmodem

which of the following are characteristics of atmuses fixed length, adds labels to data units

which four of the following are the responsibility of the wan service providerdce, co, local loop, pse

which network type divides transmitted datapacket switched

which of the following wan technologies provides packet switching over high qualityframe relay

which wan connection types use digital communications over public telephone linesdsl, isdn

which of the following is true of multiprotocol label switchingit can, cef

what is the maximum data rate of an isdn128

which of the following are characteristics of isdnit is a dial up, it provides, it lets

You have a series of wan links. What type of connection is being usedpoint to point

Which of the following devices is used on a wan to convert synchronouscsu/dsu

Your client has acquired several small companies... Which wan encapsulation method should you recommend your client useppp

RouterA is connected to RouterB through Serial1a

Two routers with the hostnames SLC and PROVOon slc, change the username password to chocolate

Which of the following statements about the functionality of lcp are truedata, lcp provides mulitlink, usernames

which of the following are benefits of lcpnegotiates, provides load, monitors

what is the connection order used by two tcplcp, authentication

ppp supports authentication, compression, and mulitiple network-layer protocolsnegotiate compression settings, perform authentication

which of the following protocols is used by ppp to enable support for multiple network-layer protocolsncp

which of the following wan technologies provides digital dial up connectionsisdn bri

a healthcare organization provides mobile clinics throughout the world. even remote areas? satellite

which of the following forms of networking are highly susceptible to eavesdroppingwireless

which of the following is most susceptible to interference related to atmospheric conditionssatellite

which of the following internet access technologies support simultaneous voiceisdn bri, adsl

which of the following internet services provides equal upload and download bandwithsdsl

which of the following are characteristics of vdslsupports both, unequal

which of the following technologies does gsm use to allowtime division

which of the following cellular network types does not provide internet2g

which of the following cellular network types use MIMO to increase 3g datalte, hspa+

Drag the cellular network specification2g: gsm, cdma. 3g: lte, hspa. 4g: wimax

which of the following describe the edge cellularoffers, the first internet

which of the following internet connection technologies requires that the location be withindsl

which of the following services are available regardlesscable modem

which type of internet service uses the DOCSIS specificationcoaxial cable

which of the following are methods for providing centralized authenticationradius, tacacs

you have decided to implement a remote access... which of the following would be a required partconfigure the remote access servers as radius clients

which of the following protocols can be used to centralize remote access authenticationtacacs

you want to set up a service to allow multiple users to dial in to the office serverras

you are configuring your computer to dial up to the internet. what protocol should you useppp

which of the following protocols or services is commonly used on cable internet connections for user authenticationpppoe

you often travel away from the office. you want the connection to be as secure as possible. which type of connection will you needremote access

you have just signed up for internet access using a local provider that gives. which of the following protocols would be used to provide authenticationpppoe

radius is primarily used for what purposeauthenticating remote clients before access to the network is granted

which of the following is a characteristic of tacacsencrypts the entire packet

which of the following ports are used with tacacs49

which type of device is required to implement port authenticationradius server

which of the following are characteristics of tacacsuses tcp, allows for a possible of 3 diff

you are troubleshooting physical layer issues with the gi0/1 interface in a routershow interfaces gi0/1

you are troubleshooting physical layer issues with the gi0/1. which commands could you use? show interfaces gi0/1 status, show interfaces gi0/1

review the output from the show interfacesa duplex mismatch

consider the network shown in exhibitcollisions are occurring

you are reviewing the output of the show interfaces command for the gi0/1. what are the most likely causes? emi, collisions

you are reviewing the output of the show interfaces. which interface statistic displays the number of collisions that occured after the 64th bytelate collisions

a workstation is connected to a switch on the gi 0/2. which of the following are true in this scenarioif the link speed is 10 half duplex is used. if the link speed is 1000 full duplex is used. the switch attempts

consider the network shown in the exhibitthe device connected to the fa0/1 interface has auto

your organization recently opened a branch office. what is the most likely cause of this poor wan performancethere is latency on the wan link

your organization recently opened a branch office. recently, your ceo conducted a video. what is the most likely cause of this poor wan performancethe wan provider

your organization recently opened a branch office. what are the most likely causes of this wan issuethere is a problem with the service provider's network. the wan interface on one or both routers

your organization recently opened a branch office. this morning, users at the branch office. you ran the show interfaces. what is the most likely causethere is a data link encapsulation

your organization recently opened a branch office. this morning. you ran the show interacesthere is an authentication misconfig

your organization recently opened a branch office. this morning. you ran the show interaces. interface up protocol upthere is an ip address misconfig

ONTESTOUT 11 SPECIFICALLY FOR YOUFOR ONLY$13. 90/PAGEOrder Now