

# [Chapter 13](https://assignbuster.com/chapter-13-2/)

WEB SERVERSCOMPUTERS RUNNING SPECIALIZED OPERATING SYSTEMS THAT ENABLE THEM TO HOST WEB PAGES AND OTHER INFORMATION ARE CALLED........

COMMERCECOMPUTERS THAT HOST SOFTWARE THAT ENABLES USERS TO PURCHASE GOODS AND SERVICES OVER THE INTERNET ARE CALLED.......... SERVERS

RECIPIENTS ADDRESS, SENDERS ADDRESS, REASSEMBLING INSTRUCTIONS, AND DATAAT A MINIMUM, WHAT CONTENT MUST ALL DAT PACKETS CONTAIN

SMTPUSED TO TRANSMIT EMAIL OVER TEH INTERNET

PACKET SWITCHINGIS THE COMMUNICATIONS METHODOLOGY WHERE DATA IS BROKEN INTO SMALLER CHUNKS TO BE SENT OVER VARIOUS ROUTES AT THE SAME TIME

CLIENT/SERVERTHE MAJORITY OF INTERNET COMMUNICATIONS FOLLOW THE....... MODEL OF NETWORK COMMUNICATIONS

STATIC ADDRESSAN IP ADDRESS THAT DOES NOT CHANGE IS USUALLY ASSIGNED MANUALLY BY A NETWORK ADMINISTRATOR

VOIPPROTOCOL USES STANDARD INTERNET CONNECTIONS TO MAKE PHONE CALLS OVER THE INTERNET

THE ADDRESSES AR 16 BIT NUMBERSCONCERNING IPV4 ADDRESSES IS FALSE

IP ADDRESSA UNIQUE NUMBER THAT IDENTIFIES A COMPUTERSERVER OR DEVICE CONNECTED TO THE INTERNET IS CALLED A ..... L

TWISTED PAIR WIRESORIGINAL INTERNET BACKBONE USED T LINES WHICH USED.....

TOP LEVEL DOMAINS. COM AND . ORG ARE EXAMPLES OF........

DYNAMIC ADDRESSA ......... IS AN IP ADDRESS THAT IS ASSIGNED FROM AN AVAILABLE POOL OF IP ADDRESSES

ICANNIS THE ORGANIZATION RESPONSIBLE FOR THE INTERNETS DOMAIN NAME SYSTEM AND IP ADDRESS ALLOCATION

BACKBONETHE MAIN PATHS OF THE INTERNET ALONG WHICH DATA TRAVELS FASTEST ARE KNOWN COLLECTIVELY AS TEH INTERNET ............

COMPUTER PROTOCOLA SET OF RULES FOR EXCHANGING ELECTRONIC INFORMATION IS CALLED A .......

MIMESIMPLIFIES ATTACHMENTS TO EMAIL MESSAGES

HYPERTEXT DOCUMENTA...... CONTAINS TEXT THAT IS LINKED TO OTHER DOCUMENTS OR MEDIA

OPEN SYSTEMSTANDARDS THAT ARE MADE PUBLIC FOR ACCESS BY ANY INTERESTED PARTY ARE CALLED........ PROTOCOLS

TCP/IPTHE MAIN SUITE OF PROTOCOLS USED ON THE INTERNET IS..........................

HYPERLINKSHYPERTEXT DOCUMENTS CONTAIN............ THAT YOU CAN CLICK ON AND THAT LINK THE DOCUMENT TO OTHER DOCUMENTS OR MEDIA

NETWORK PREFIXCIDR ALLOWS A SINGLE IP ADDRESS TO REPRESENT SEVERAL UNIQUE IP ADDRESSES BY ADDING A .......... TO THE END OF THE LAST OCTET

ONCHAPTER 13 SPECIFICALLY FOR YOUFOR ONLY$13. 90/PAGEOrder Now