

# [Cs 8 ch7-9](https://assignbuster.com/cs-8-ch7-9/)

ARPANETThe original Internet was called

FTTHThe broadband Internet service that runs over fiber optic cable is:

ISPA(n)\_\_\_\_\_\_ is a company that offers Internet access.

SafariThe default Web browser on a Mac is:

TabsYou can view multiple Web pages in most browsers using:

add-onA(n) \_\_\_ is a third-party program that extends the functionality of a Web browser.

TLD (top- level domain)Examples of \_\_\_\_\_ include . com, . gov, and . edu

DNS (Domain Name System)The \_\_\_\_ allows you to type a URL in your browser instead of an IP address.

restrictedOne way to evaluate a website’s credibility is to look for a \_\_\_ TLD

About Us PageCheck the \_\_\_\_\_\_ on a website for the credentials of the author or organization.

Internet BackboneThe \_\_\_\_\_\_\_ is the high- speed connection point between networks

hyperlinkThe \_\_\_\_\_ is the part of the Internet that uses hypertext to connect pieces of information.

DSL\_\_\_\_\_\_ is broadband over digital telephone lines

broadbandInternet access that exceeds 200 kbps is considered \_\_\_

LTE, WiMAXThe two formats of 4G Internet access are \_\_\_\_ and \_\_\_

HTMLBasic Web pages are written in \_\_\_

web browsersInternet Explorer, Firefox, and Safari are examples of \_\_\_\_\_\_\_

home pageThe \_\_\_\_\_\_ is the Web page that appears when you open your browser

URLAnother term for the address of a website is \_\_\_\_

TLDThe \_\_\_\_ . gov is restricted to government websites.

Instant messagingWhat form of online communication happens in real time between two people?

ChatsWhat are synchronous online conversations between multiple people a the same time?

store-and-forwardEmail is a \_\_\_\_\_ form of online communication

Bcc: Which field prevents multiple recipients from seeing each other’s email address?

MMORPGA(n) \_\_\_\_ is an online game in which players interact with people in real time in a virtual world using an avatar.

social networksFacebook and LinkedIn are examples of:

digital footprintYour \_\_\_\_\_ is all the information that someone could find out about you by searching the Web, including social network sites.

RSSWhat service is used to distribute Web feeds to subscribers?

MicroblogIn which type of social media are past limited to a small number of characters and uses post updates frequently?

SMM\_\_\_\_ is the practice of using social media sites to sell products and service.

Synchronous\_\_\_ online communication happens in real time

forumA \_\_\_\_, or discussion board, is an asynchronous form of communication

captchaA(n) \_\_\_\_ is a series of letters and numbers that are distorted in some way

Web 2. 0New technologies used to communicate and collaborate on the Web are called \_\_\_\_

digital footprintYour \_\_\_\_\_ is all the information that someone would find out about you by searching the Web, including social network sites

blogosphereThe \_\_\_\_\_ consists of all the blogs on the Web and the connections between them

RSS\_\_\_\_\_ is a format used for distributing Web funds that change frequently- for example, blogs, podcasts, and news-to subscribers

podcastA(n) \_\_\_\_ is a digital media file of a prerecorded radio- or TV- like show that is distributed over the Web

Social bookmarking\_\_\_\_\_\_ sites allow you to save and share your favorites online

E- commerence\_\_\_\_\_\_\_ is doing business on the Web.

workgroupComputers in a peer-to-peer network belong to a \_\_\_\_

DocumentsWhich resources are not shared by default in a homegroup?

SANWhich type of network consists of data storage devices and servers?

WANWhich type of network spans multiple locations and connects multiple network?

BusWhich topology connects devices in a single line?

Personal area network (PAN)When two Bluetooth devices connect to each other directly, they form a(n) \_\_\_\_\_.

routerThe device needed to connect two or more networks together is called a(n) \_\_\_\_\_

switchA(n) \_\_\_\_\_ connects multiple devices on LAN

TCPWhich protocol is responsible for assuming that data packets are transmitted reliably on a network?

FirewallWhich device examines data packets as they enter and leave a network and denies unauthorized packet access?

Network resources\_\_\_\_\_ include software, hardware, and files

VPNA(n) \_\_\_\_ creates a private network through a public network

client- server networkA(n) \_\_\_\_\_\_ has at least one server at its center

infrastructure wireless networkIn a(n) \_\_\_\_\_\_\_, devices connect through a wireless access point

LANA(n) \_\_\_ is a network that has all devices located in the same physical location

Topology\_\_\_\_ is the physical layout of a local area network

network adapterEvery device on a network must have a(n) \_\_\_\_\_ to establish a connection with a network

modemAn analog \_\_\_\_ is the first device on a network that connects to the Internet via telephone lines

domainA group of clients and servers under the control of one central security database us called a(n):

Protocols\_\_\_\_ define the rates for communication between devices